ITEM #: STARTER STATION  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.  
Fabricate and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation with Item #, Chef’s Counter with Sink.  
4. Provide two (2) tiered unit with top tier at no taller than 66" at the peak.  
5. Top tier shall be slanted and able to accept 1/3rd size or 1/6th size hotel pans with proper adaptor bars provided.  
6. Lower Tier shall be able to accept 1/3rd size or 1/6th size hotel pans with proper adaptor bars provided.  
7. Provide full complement of pans with the starter station.  
8. Coordinate installation over Item #, Tray Lowerator Dispenser.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.