ITEM #: STEAM SYSTEM  
Quantity: One (1)  
Manufacturer: Modbar  
Model No.: Steam System  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH; 12.0A; 1/2" CW  
  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide dual wall cool-touch wand.  
4. Provide pid temperature control.  
5. Provide USB update port.  
6. Provide touch screen controls.  
7. Provide linea style porthole sight glass.  
8. Unit able to powers one or two taps per module.  
9. Provide 10-min start up time from cold.  
10. Coordinate installation onto Item #, Service Prep Counter with Sink and Glass Polishing Station.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.