ITEM #: TURBO OVEN  
Quantity: One (1)  
Manufacturer: Turbo Chef   
Model No.: i5  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH, 46.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide stainless steel type 304 oven liner.  
3. Provide integral recirculating catalytic converter.  
4. Provide independently controlled dual motors for vertically recirculated air impingement.  
5. Provide heavy duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
6. Coordinate installation onto Item #, Freezer Base.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.