ITEM # : UNDERCOUNTER FREEZER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: HB24FS4  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH, 2.4A   
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide four (4) 2-7/8” casters.  
4. Provide heavy-duty cord and plug.  
5. Provide unit with (2) stainless steel drawers with locks.  
6. Provide two wine drawers with upper basket and two doors hinged as shown on plan.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.