ITEM #: UNDERCOUNTER FREEZER  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: TUC-24F-HC  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH, 2.3A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have stainless steel door fitted with a 12” long recessed handle that is foamed in place with a sheet metal interlock.  
3. Unit shall have all stainless steel front, top, and ends.  
4. Unit interior shall be constructed of NSF approved clear coated aluminum liner with a stainless steel floor.  
5. Equip the doors with locks.  
6. Provide heavy duty PVC coated gray wire shelves.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.