ITEM #: UNDERCOUNTER FREEZER   
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: TUC-60F-LP-HC~SPEC1  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 3.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with 1-1/2" high, heavy duty, polyurethane, casters, two (2) with brakes.   
3. Coordinate installation under Item #  
4. Provide unit with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.  
5. Provide low profile model with 31-7/8" work surface height.  
6. Provide additional Shelves.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.