ITEM #: UNDERCOUNTER ICE MACHINE WITH BIN  
Quantity: Two (2)  
Manufacturer: Scotsman  
Model No.: CU1526MA-1  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 15.0A; 3/8" CW; 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide an AutoAlertJ control panel which can communicate operating status and signal when it’s time to descale, and sanitize.  
4. Provide unit with an ice scoop.  
5. Provide unit with 6" adjustable legs.  
6. Provide a 6' heavy duty cord and plug. Coordinate NEMA configuration with the Electrical Contractor.  
7. Ice machine shall produce medium cube ice 7/8A x 7/8" x 7/8".  
8. The bin shall have an 80 lb capacity.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.