ITEM #: UNDERCOUNTER ICE MACHINE& BIN  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: UF0915A-1  
Pertinent Data: 90 Pounds ARI Capacity, Air Cooled; Future Equipment  
Utilities Req’d: 120V/1PH, 15.0A; 3/8” CW, 3/4” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Ice Maker shall produce up to 99 lb per day and bin can store 36 lb.  
5. Ice maker shall produce flake ice.  
6. Provide unit with KUFM15 floor mount kit to lower the overall height to 31.9”.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.