ITEM #: UNDERCOUNTER ICE MAKER  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: IM-50BAA-LM  
Pertinent Data: 50 Pounds/22.7 kG Capacity, Air Cooled  
Utilities Req'd: 208V/1PH, 5.0A; 1/2" CW, 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Provide the connection between ice machine and Item #\_\_\_\_\_\_, Water Filtration System.  
4. Ice maker shall contain bin with 22 pounds/10kg storage capacity.  
5. Ice machine shall produce square cubes 2.3" x 1.9" x 1.9" (58.4mm x 48.3mm x 48.3mm).  
6. Ensure that Ice Maker fits under Item #\_\_\_  
7. Must meet all applicable governmental, and local laws, rules, regulations, and codes.