ITEM #: VEGETABLE SLICER  
Quantity: One (1)  
Manufacturer: Piper Products  
Model No.: GSM XL  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 14.5A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with heavy-duty cord and plug. Coordinate NEMA configuration with Electrical Contractor.  
3. Provide the following processing plates:  
 G35 1/8” slicing plate, and G105 5/8” slicing plate.  
4. Coordinate installation onto Item #, Cold Preparation Table with Sink.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.