ITEM #: WALL CABINET  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS\_\_\_\_\_  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FS\_\_\_.1, Detail #6.  
2. Size and configuration as shown on drawings.  
3. Set in place in location as shown on drawings.  
4. Coordinate installation above Item #\_\_\_\_\_\_\_\_  
5. Provide hinged stainless steel doors with integrally formed full length door pull and intermediate shelves.  
6. All finished edges shall be #7 mirrored polish finish.  
7. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.  
8. Provide shop drawings for approval prior to fabrication.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.