ITEM #: WHITE WINE REFRIGERATOR  
Quantity: One (1)  
Manufacturer: EuroCave  
Model No.: E-Pure-L  
Pertinent Data: Single Section, Self-Contained  
Utilities Req’d: 120V/1PH; 3.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with three (3) temperatures.  
4. Unit shall have glass doors with silver frames hinged right.  
5. Provide a handle that is integrated to the door frame.  
6. Provide unit with 10 sliding shelves.  
7. Equip unit with amber LED lights.  
8. Provide with heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
9. Unit shall be equipped with door locks.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.