TEM #337: FOOD WARMER  
Quantity: One (1)  
Manufacturer: Hatco  
Model No.: GRAH-30  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 5.5A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide infinite controls and remote-control enclosure. Food warmer controls shall be installed on counter apron.  
3. Provide indicator light.  
4. Coordinate installation onto Item #\_\_\_.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.