**PREPARATION AREA**

ITEM #1: PREPARATION TABLE WITH SINKS (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #2: SPARE NUMBER

ITEM #3: DOUBLE WALL SHELF (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #4: PRE-RINSE UNIT (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: WITH FAUCET, EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #5: SPARE NUMBER

ITEM #6: DOUBLE WALL SHELF (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #7: TRASH RECEPTACLE (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: WITH LID AND DOLLY, EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #8: INGREDIENT BIN (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG360088  
Pertinent Data: MOBILE, EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #9: SPARE NUMBER

ITEM #10: SPARE NUMBER

ITEM #11: DOUBLE WALL SHELF (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #12: SPARE NUMBER

ITEM #13: SPARE NUMBER

ITEM #14: PREPARATION COOLER  
Quantity: One (1)  
Manufacturer: THERMALRITE  
Model No.: CUSTOM  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 20.0A (FOR LIGHTS & DOOR HEATER)

ITEM #15: SPARE NUMBER

ITEM #16: FLOOR TROUGH & GRATE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: 2" drain recessed 4"

ITEM #17: EVAPORATOR COIL  
Quantity: One (1)  
Manufacturer: RDT  
Model No.: BEL0095  
Pertinent Data: ON EMERGENCY POWER  
Utilities Req'd: 120V/1PH, 1.8A (ON EMERGENCY POWER / DATA CABLE REQUIRED); 3/4" IW

ITEM #18: COOLER STORAGE SHELVING  
Quantity: Seven (7)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: MOBILE, FIVE TIER  
Utilities Req'd: ---

ITEM #19: SPARE NUMBER

ITEM #20: SPARE NUMBER

ITEM #21: PREPARATION TABLE (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #22: SPARE NUMBER

ITEM #23: TRASH RECEPTACLE (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: WITH LID AND DOLLY, EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #24: SPARE NUMBER

ITEM #25: SPARE NUMBER

ITEM #26: HAND SINK (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-68  
Pertinent Data: WITH VENDOR PROVIDED SOAP & TOWEL DISPENSER, EXISTING TO REMAIN  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with gooseneck faucet.  
3. Provide unit with p trap and tail piece.  
4. Provide battery-operated faucet. (K-175 swing spout faucet).  
5. Provide 6 Volt battery to operate electronic sensor.  
6. Provide 12” welded side splash on each side 7-PS-11.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #27: SPARE NUMBER

ITEM #28: SPARE NUMBER

ITEM #29: SPARE NUMBER

ITEM #30: SPARE NUMBER

**WAREWASHING AREA**

ITEM #31: POT SINK (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #32: POT SHELF (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #33: TRASH RECEPTACLE (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: WITH LID AND DOLLY, EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #34: SPARE NUMBER

ITEM #35: DISPOSER (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #36: FLOOR TROUGH & GRATE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: 2" drain recessed 4"

ITEM #37: HOSE REEL (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: FISHER  
Model No.: 75222  
Pertinent Data: CEILING MOUNT - EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #38: SPARE NUMBER

ITEM #39: SPARE NUMBER

ITEM #40: SPARE NUMBER

ITEM #41: HOSE REEL CONTROL CABINET (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: FOR ITEM #37, EXISTING TO RELOCATE  
Utilities Req'd: 1/2" CW, 1/2" HW

ITEM #42: POT AND PAN SHELVING  
Quantity: Five (5)  
Manufacturer: METRO  
Model No.: MAX4  
Pertinent Data: MOBILE, FOUR TIER  
Utilities Req'd: ---

ITEM #43: MOP SINK (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY GENERAL CONTRACTOR

ITEM #44: HOSE BIBB (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY GENERAL CONTRACTOR

ITEM #45: SPARE NUMBER

ITEM #46: WALL SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #47: REVERSE OSMOSIS SYSTEM (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: FOR ITEM #87, EXISTING TO RELOCATE  
Utilities Req'd: 3/8" CW, 1/4" IW

ITEM #48: REVERSE OSMOSIS STORAGE TANK (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: FOR ITEM #47, EXISTING TO RELOCATE  
Utilities Req'd: 1/2" CW

ITEM #49: DETERGENT STORAGE SHELVING  
Quantity: One (1)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: FIXED, FIVE TIER  
Utilities Req'd: ---

ITEM #50: SPARE NUMBER

ITEM #51: MOP RACK (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY GENERAL CONTRACTOR

ITEM #52: SPARE NUMBER

ITEM #53: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #54: HAND SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-61  
Pertinent Data: WITH VENDOR PROVIDED SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

ITEM #55: SPARE NUMBER

ITEM #56: SOILED DISH TABLE WITH SINK  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: 1-1/2" IW

ITEM #57: DOUBLE SIDED GLASS RACK SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #56  
Utilities Req'd: ---

ITEM #58: DISH DROP WINDOW WITH SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #59: SILVERWARE CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #60: SILVER SOAK SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 9-FSS-20  
Pertinent Data: MOBILE  
Utilities Req'd: ---

ITEM #61: SPARE NUMBER

ITEM #62: TRASH RECEPTACLE (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG262000GRAY  
Pertinent Data: WITH LID AND DOLLY, EXISTING TO RELOCATE  
Utilities Req'd: ---

ITEM #63: FLOOR TROUGH & GRATE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: 2" drain recessed 4"

ITEM #64: HOSE REEL (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: FISHER  
Model No.: 75222  
Pertinent Data: CEILING MOUNT, EXISTING TO RELOCATE  
Utilities Req'd: ---

ITEM #65: SPARE NUMBER

ITEM #66: HOSE REEL CONTROL CABINET (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: FOR ITEM #64, EXISTING TO RELOCATE  
Utilities Req'd: 1/2" CW, 1/2" HW

ITEM #67: PRE-RINSE UNIT  
Quantity: One (1)  
Manufacturer: FISHER  
Model No.: 34460  
Pertinent Data: WITH FAUCET  
Utilities Req'd: 1/2" CW, 1/2" HW

ITEM #68: DISH MACHINE (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: HOBART  
Model No.: CLPS66e  
Pertinent Data: EXISTING TO RELOCATE  
Utilities Req'd: 208V/3PH, 138.9A; 1/2" HW, 2" IW

ITEM #69: SPARE NUMBER

ITEM #70: SPARE NUMBER

ITEM #71: CLEAN DISH TABLE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #72: UNDERCOUNTER DISH MACHINE  
Quantity: One (1)  
Manufacturer: ELECTROLUX  
Model No.: 502315  
Pertinent Data: ---  
Utilities Req'd: 208V/3PH, 19.0A; 3/4" HW, 3/4" IW

ITEM #73: GLASS RACK SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: WALL MOUNTED  
Utilities Req'd: ---

ITEM #74: SPARE NUMBER

ITEM #75: SPARE NUMBER

ITEM #76: DRY STORAGE SHELVING (EXISTING EQUIPMENT)  
Quantity: Five (5)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: FIXED, FIVE TIER, EXISTING TO RELOCATE  
Utilities Req'd: ---

ITEM #77: DRY STORAGE SHELVING  
Quantity: Three (3)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: FIXED, FIVE TIER  
Utilities Req'd: ---

ITEM #78: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #79: SPARE NUMBER

ITEM #80: SPARE NUMBER

ITEM #81: HAND SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-61  
Pertinent Data: WITH VENDOR PROVIDED SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

ITEM #82: SPARE NUMBER

ITEM #83: SPARE NUMBER

ITEM #84: SPARE NUMBER

ITEM #85: SPARE NUMBER

**REMOTE EQUIPMENT AREA**

ITEM #86: REFRIGERATION RACK  
Quantity: One (1)  
Manufacturer: RDT  
Model No.: IRW1-02Z-CT3-AST  
Pertinent Data: OUTDOOR, AIR-COOLED, ON EMERGENCY POWER  
Utilities Req'd: 208V/1PH, 19.5A

ITEM #87: COMBI OVEN W/ STAND (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ---  
Model No.: ---  
Pertinent Data: MOBILE, EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #88: SPARE NUMBER

ITEM #89: SPARE NUMBER

ITEM #90-100: SPARE NUMBERS

**COOKING AREA**

ITEM #101: DRY STORAGE SHELVING  
Quantity: Two (2)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: FIXED, FIVE TIER  
Utilities Req'd: ---

ITEM #102: CHEF'S COOLER  
Quantity: One (1)  
Manufacturer: THERMALRITE  
Model No.: CUSTOM  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 20.0A (FOR LIGHTS & DOOR HEATER)

ITEM #103: EVAPORATOR COIL  
Quantity: One (1)  
Manufacturer: RDT  
Model No.: BEL0095  
Pertinent Data: ON EMERGENCY POWER  
Utilities Req'd: 120V/1PH, 1.8A (ON EMERGENCY POWER / DATA CABLE REQUIRED); 3/4" IW

ITEM #104: COOLER STORAGE SHELVING  
Quantity: Six (6)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: MOBILE, FIVE TIER  
Utilities Req'd: ---

ITEM #105: FLOOR TROUGH & GRATE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: 2" drain recessed 4"

ITEM #106: DISPLAY COOLER SHELVING  
Quantity: One (1)  
Manufacturer: ANTHONY  
Model No.: GFS 91611  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #107: DISPLAY COOLER DOOR  
Quantity: One (1)  
Manufacturer: ANTHONY  
Model No.: INFINITY-60  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #108: CHEF'S COUNTER WITH SINK  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: (2) 120V/1PH, 20.0A (CONVENIENCE OUTLETS); 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #109: DOUBLE OVERSHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #110: FOOD WARMER  
Quantity: One (1)  
Manufacturer: HATCO  
Model No.: GRAH-54  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 10.4A

ITEM #111: DROP-IN HAND SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-42  
Pertinent Data: WITH SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with gooseneck faucet.  
3. Provide with c fold towel dispenser.  
4. Provide unit with p trap and tail piece.  
5. Provide unit with wrist blade.  
6. Coordinate installation into Item #1501, Back Counter as shown on drawings.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #112: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #108  
Utilities Req'd: ---

ITEM #113: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #114: UNDERCOUNTER FREEZER  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: SWF27N-U-D  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 4.0A

ITEM #115: FOOD WARMER  
Quantity: One (1)  
Manufacturer: HATCO  
Model No.: GRAH-60  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 11.7A

ITEM #116: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #117: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: SW36N-U  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 6.3A

ITEM #118: RECESSED CUTTING BOARD  
Quantity: Two (2)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #108  
Utilities Req'd: ---

ITEM #119: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: D48N-U-D  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 2.5A

ITEM #120: FOOD WARMER  
Quantity: Two (2)  
Manufacturer: HATCO  
Model No.: GRAH-42  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 7.9A

ITEM #121: HOT FOOD WELL  
Quantity: One (1)  
Manufacturer: WELLS  
Model No.: MOD-300TDM/AF  
Pertinent Data: 3 WELL, AUTOFILL  
Utilities Req'd: 208V/1PH, 17.9A; 1/2" HW, 1" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide factory installed drain manifold, and auto fill.  
3. Provide drain valve extension kit and drain screens.  
4. Hot food well controls shall be installed on counter apron.  
5. Unit shall be pre-wired to controls on apron.  
6. Coordinate installation onto Item #327, Plating Table.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #122: RECESSED CUTTING BOARD  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #108  
Utilities Req'd: ---

ITEM #123: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #124: LOAD CENTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: 120/208V/1PH, 85.0A (E.C. TO VERIFY LOAD)

ITEM #125: SPARE NUMBER

ITEM #126: EXHAUST HOOD  
Quantity: One (1)  
Manufacturer: GAYLORD  
Model No.: ELX  
Pertinent Data: WITH MAKE-UP AIR  
Utilities Req'd: 120V/1PH, 20.0A (FOR LIGHTS); 3450 CFM Exhaust, 2898 CFM Exhaust, 1380 CFM Supply, 1159 CFM Supply

ITEM #127: DUMP STATION  
Quantity: One (1)  
Manufacturer: ULTRAFRYER  
Model No.: 11D911  
Pertinent Data: MOBILE, WITH HEAT LAMP  
Utilities Req'd: 120V/1PH, 15A

ITEM #128: FRYER BATTERY  
Quantity: One (1)  
Manufacturer: ULTRAFRYER  
Model No.: B-P20-18-2-UCP  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 8.5A; 3/4" Gas @ 130000 BTU; 7" WC

ITEM #129: PLATE SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #108  
Utilities Req'd: ---

ITEM #130: SPARE NUMBER

ITEM #131: SPREADER  
Quantity: One (1)  
Manufacturer: JADE  
Model No.: JMPR-6  
Pertinent Data: MOBILE  
Utilities Req'd: ---

ITEM #132: GRIDDLE  
Quantity: One (1)  
Manufacturer: JADE   
Model No.: JMRH-36G  
Pertinent Data: ---  
Utilities Req'd: 3/4" Gas @ 105000 BTU; 5" WC

ITEM #133: MODULAR FOUR BURNER RANGE  
Quantity: Two (2)  
Manufacturer: JADE  
Model No.: JMRH-4  
Pertinent Data: ---  
Utilities Req'd: 3/4" Gas @ 140000 BTU; 5" WC

ITEM #134: SALAMANDER  
Quantity: Two (2)  
Manufacturer: JADE  
Model No.: JSB-36  
Pertinent Data: WALL MOUNTED  
Utilities Req'd: 3/4" Gas @ 35000 BTU; 5" WC

ITEM #135: SPARE NUMBER

ITEM #136: REFRIGERATED EQUIPMENT STAND  
Quantity: One (1)  
Manufacturer: JADE  
Model No.: JRLH-04S-T-72  
Pertinent Data: MOBILE, MODULAR  
Utilities Req'd: 120V/1PH, 12.6A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Units construction shall be cabinet interiors, front, face and sides to be stainless steel.  
3. Equip drawer faces to have flush mount pull handle. Face and back to be stainless steel, and be self-closing drawers which have 14-gauge stainless steel drawer track, with 2" heavy-duty skate wheel.  
4. Provide heavy-duty rubber drawer gaskets.  
5. Provide with heavy-duty cord and plug. Coordinate NEMA configuration with Electrical Contractor.  
6. Equip with drawers which are to be easily removable for cleaning, and to accommodate 6" deep 12" x 20" hotel pans.  
7. Provide face mounted dial thermometers.  
8. Equip unit with a Condensing unit that uses R-404 refrigerant unless otherwise specified and a blower coil evaporator with R-404 expansion valve.  
9. Provide Six (6) 6” heavy-duty, non-marking casters, front two (2) with brakes.  
10. Coordinate installation of Item #???, ???? on top of unit.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #137: CHARBROILER  
Quantity: One (1)  
Manufacturer: JADE  
Model No.: JB-54  
Pertinent Data: GAS  
Utilities Req'd: 3/4" Gas @ 105000 BTU; 5" WC

ITEM #138: REFRIGERATED EQUIPMENT STAND  
Quantity: One (1)  
Manufacturer: JADE PRODUCTS  
Model No.: JRLH-02S-T-60  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 12.6A

ITEM #139: SPARE NUMBER

ITEM #140: SPARE NUMBER

ITEM #141: MODULAR SPREADER  
Quantity: One (1)  
Manufacturer: JADE  
Model No.: JMPR-6  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #142: DOUBLE CONVECTION OVEN  
Quantity: One (1)  
Manufacturer: BLODGETT  
Model No.: MARK V-100 DBL  
Pertinent Data: MOBILE  
Utilities Req'd: (2) 208V/3PH, 30.5A

ITEM #143: FIRE SUPPRESSION SYSTEM  
Quantity: One (1)  
Manufacturer: ANSUL  
Model No.: R-102  
Pertinent Data: FOR ITEM #126  
Utilities Req'd: 120V/1PH, 20.0A (DEDICATED CIRCUIT)

ITEM #144: PREPARATION COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: (2) 120V/1PH, 20.0A (CONVENIENCE OUTLETS)

ITEM #145: SPARE NUMBER

ITEM #146: DROP-IN HAND SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-42  
Pertinent Data: WITH SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with gooseneck faucet.  
3. Provide with c fold towel dispenser.  
4. Provide unit with p trap and tail piece.  
5. Provide unit with wrist blade.  
6. Coordinate installation into Item #1501, Back Counter as shown on drawings.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #147: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #144  
Utilities Req'd: ---

ITEM #148: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #149: SPARE NUMBER

ITEM #150: SPARE NUMBER

ITEM #151: SPARE NUMBER

ITEM #152: DIPPERWELL  
Quantity: One (1)  
Manufacturer: FISHER  
Model No.: 3041  
Pertinent Data: ---  
Utilities Req'd: 1/2" HW, 1-1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a stainless steel dipper well faucet.  
4. Provide a stainless steel sink pan with a removable inner shell.  
5. Coordinate installation into Item #N456, Beverage Counter.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #153: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: D48N-U  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 2.5A

ITEM #154: DOUBLE WALL SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #155: SPARE NUMBER

ITEM #156: UNDERCOUNTER FREEZER  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: SWF27-U-D  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 4.0A

ITEM #157: DOUBLE OVERSHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #158: SANDWICH PREP REFRIGERATOR  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: SW72N18-FB-D  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 6.1A

ITEM #159: SPARE NUMBER

ITEM #160: SPARE NUMBER

ITEM #161: PLATE SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #144  
Utilities Req'd: ---

ITEM #162: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #163: REACH-IN REFRIGERATOR  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: 2RD-SD  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 6.9A

ITEM #164: BEVERAGE COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: (2) 120V/1PH, 20.0A (CONVENIENCE OUTLETS); 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #165: SPARE NUMBER

ITEM #166: SODA & ICE DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #167: ICE MACHINE  
Quantity: One (1)  
Manufacturer: SCOTSMAN  
Model No.: N0922W-32  
Pertinent Data: 900LB., WATER-COOLED, NUGGET ICE  
Utilities Req'd: 208V/1PH, 12.0A; 3/8" CW, 3/4" IW; 38" Chilled Water Supply, 1/2" Chilled Water Return

ITEM #168: WATER FILTRATION SYSTEM  
Quantity: One (1)  
Manufacturer: SCOTSMAN  
Model No.: AP2-P  
Pertinent Data: FOR ITEM #167  
Utilities Req'd: 3/4" CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate installation of Item #2604, Ice Machine.  
3. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #169: SPARE NUMBER

ITEM #170: SPARE NUMBER

ITEM #171: WATER DISPENSER  
Quantity: One (1)  
Manufacturer: ELKAY  
Model No.: DSC2K  
Pertinent Data: 2 TAP  
Utilities Req'd: ---

ITEM #172: CARBONATION CHILLER  
Quantity: One (1)  
Manufacturer: ELKAY  
Model No.: DSFBF180K  
Pertinent Data: ---  
Utilities Req'd: 3/8" CW

ITEM #173: HOT WATER DISPENSER  
Quantity: One (1)  
Manufacturer: BUNN  
Model No.: HW2  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 15.0A; 1/4" CW

ITEM #174: COFFEE BREWER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #175: SPARE NUMBER

ITEM #176: DOUBLE WALL SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #177: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #164  
Utilities Req'd: ---

ITEM #178: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #179: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True  
Model No.: TUC-27-HC  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 2.0A

ITEM #180: SPARE NUMBER

ITEM #181: GLASS RACK DISH DOLLY  
Quantity: Two (2)  
Manufacturer: METRO  
Model No.: CBH2121C  
Pertinent Data: MOBILE  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set-in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with heavy-duty, non-marking swivel casters.  
3. Provide a tubular steel handle and non-marking corner bumpers.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #182: HAND SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-61  
Pertinent Data: WITH VENDOR PROVIDED SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

ITEM #183: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #184: HOOD CONTROL CABINET  
Quantity: One (1)  
Manufacturer: GAYLORD  
Model No.: COMMAND CENTER  
Pertinent Data: FOR ITEM #126  
Utilities Req'd: 120V/1PH, 4.0A

ITEM #185: UTILITY RACK  
Quantity: Two (2)  
Manufacturer: NEW AGE  
Model No.: 1305  
Pertinent Data: MOBILE  
Utilities Req'd: ---

ITEM #186: BEVERAGE COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: (2) 120V/1PH, 20.0A (CONVENIENCE OUTLETS); 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #187: SODA & ICE DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #188: ICE MACHINE  
Quantity: One (1)  
Manufacturer: SCOTSMAN  
Model No.: N0922W-32  
Pertinent Data: 900LB., WATER-COOLED, NUGGET ICE  
Utilities Req'd: 208V/1PH, 12.0A; 3/8" CW, 3/4" IW; 38" Chilled Water Supply, 1/2" Chilled Water Return

ITEM #189: PLATING TABLE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: (2) 120V/1PH, 20.0A (CONVENIENCE OUTLETS)

ITEM #190: HEATED CABINET  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: DL1W-SS-HD  
Pertinent Data: MOBILE  
Utilities Req'd: 208/230V/1PH, 7.2A

ITEM #191: WATER FILTRATION SYSTEM  
Quantity: One (1)  
Manufacturer: SCOTSMAN  
Model No.: AP2-P  
Pertinent Data: FOR ITEM #188  
Utilities Req'd: 3/4" CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate installation of Item #2604, Ice Machine.  
3. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #192: TRASH RECEPTACLE  
Quantity: Two (2)  
Manufacturer: RUBBERMAID  
Model No.: FG262000GRAY  
Pertinent Data: WITH LID AND DOLLY  
Utilities Req'd: ---

ITEM #193: ICED TEA BREWER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #194: COFFEE BREWER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #195: GLASS RACK DISH DOLLY  
Quantity: Three (3)  
Manufacturer: METRO  
Model No.: CBH2121C  
Pertinent Data: MOBILE  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set-in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with heavy-duty, non-marking swivel casters.  
3. Provide a tubular steel handle and non-marking corner bumpers.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #196: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG262000GRAY  
Pertinent Data: WITH LID AND DOLLY  
Utilities Req'd: ---

ITEM #197: HAND SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-61  
Pertinent Data: WITH VENDOR PROVIDED SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

ITEM #198: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #199: DRY STORAGE SHELVING  
Quantity: Three (3)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: FIXED, FIVE TIER  
Utilities Req'd: ---

ITEM #200: SPARE NUMBER

**BEVERAGE AREA**

ITEM #201: MOP SINK CABINET  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 9-OPC-84  
Pertinent Data: ---  
Utilities Req'd: 1/2" CW, 1/2" HW, 2" DW

ITEM #202: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #203: HAND SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-61  
Pertinent Data: WITH VENDOR PROVIDED SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

ITEM #204: SODA SYSTEM AND RACK (NOT IN CONTRACT)  
Quantity: Two (2)  
Pertinent Data: BY VENDOR

ITEM #205: SPARE NUMBER

ITEM #206: DRY STORAGE SHELVING  
Quantity: Six (6)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: FIXED, FIVE TIER  
Utilities Req'd: ---

ITEM #207: SPARE NUMBER

ITEM #208: SPARE NUMBER

ITEM #209: SPARE NUMBER

ITEM #210: SPARE NUMBER

ITEM #211: BEVERAGE COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: (2) 120V/1PH, 20.0A (CONVENIENCE OUTLETS)

ITEM #212: CUP DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #213: SODA AND ICE DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #214: ICE MACHINE  
Quantity: One (1)  
Manufacturer: SCOTSMAN  
Model No.: NH0922W-32  
Pertinent Data: 900LB., WATER-COOLED, NUGGET ICE  
Utilities Req'd: 208V/1PH, 12.0A; 3/8" CW, 3/4" IW; 38" Chilled Water Supply, 1/2" Chilled Water Return

ITEM #215: SPARE NUMBER

ITEM #216: CUP DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #217: WATER FILTRATION SYSTEM  
Quantity: One (1)  
Manufacturer: EVERPURE  
Model No.: EV9275-01  
Pertinent Data: FOR ITEM #214 & #218  
Utilities Req'd: 3/8" CW

ITEM #218: LIQUID COFFEE DISPENSER  
Quantity: One (1)  
Manufacturer: BUNN  
Model No.: LCS-2 (34400.0001)  
Pertinent Data: ---  
Utilities Req'd: 120/208V/1PH, 13.2A; 3/8" CW

ITEM #219: SPARE NUMBER

ITEM #220: SPARE NUMBER

ITEM #221: CUP DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #222: SPARE NUMBER

ITEM #223: SPARE NUMBER

ITEM #224: SPARE NUMBER

ITEM #225: SPARE NUMBER

ITEM #226: SPARE NUMBER

ITEM #227: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #211  
Utilities Req'd: ---

ITEM #228: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #229: SPARE NUMBER

ITEM #230: SPARE NUMBER

ITEM #231: SPARE NUMBER

ITEM #232: WALL CABINET (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #233: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #211  
Utilities Req'd: ---

ITEM #234: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #235: SPARE NUMBER

ITEM #236: SPARE NUMBER

ITEM #237: SPARE NUMBER

ITEM #238: SPARE NUMBER

ITEM #239: SPARE NUMBER

ITEM #240: SPARE NUMBER

ITEM #241: SPARE NUMBER

ITEM #242: CUP DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #243: LIQUID COFFEE DISPENSER  
Quantity: One (1)  
Manufacturer: BUNN  
Model No.: LCS-2 (34400.0001)  
Pertinent Data: ---  
Utilities Req'd: 120/208V/1PH, 13.2A; 3/8" CW

ITEM #244: WATER FILTRATION SYSTEM  
Quantity: One (1)  
Manufacturer: EVERPURE  
Model No.: EV9275-01  
Pertinent Data: FOR ITEM #243 & #248  
Utilities Req'd: 3/8" CW

ITEM #245: SPARE NUMBER

ITEM #246: CUP DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #247: SODA AND ICE DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #248: ICE MACHINE  
Quantity: One (1)  
Manufacturer: SCOTSMAN  
Model No.: NH0922W-32  
Pertinent Data: 900LB., WATER-COOLED, NUGGET ICE  
Utilities Req'd: 208V/1PH, 12.0A; 3/8" CW, 3/4" IW; 38" Chilled Water Supply, 1/2" Chilled Water Return

ITEM #249: SPARE NUMBER

ITEM #250: SPARE NUMBER

ITEM #251: CUP DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #252: SPARE NUMBER

ITEM #253: SPARE NUMBER

ITEM #254: SPARE NUMBER

ITEM #255-300: SPARE NUMBERS

**COFFEE BAR AREA**

ITEM #301: SWING GATE (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #302: BARISTA COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #303: REFRIGERATED DISPLAY CASE  
Quantity: One (1)  
Manufacturer: STRUCTURAL CONCEPTS  
Model No.: NR6055RSV  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #304: AMBIENT GRAB-N-GO CASE  
Quantity: One (1)  
Manufacturer: STRUCTURAL CONCEPT  
Model No.: NR3635DSV  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 2.0A

ITEM #305: BARISTA COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #306: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: D48N-U  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 2.5A

ITEM #307: POS SYSTEM (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #308: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #309: SPARE NUMBER

ITEM #310: SPARE NUMBER

ITEM #311: OPEN SHELVING  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #301  
Utilities Req'd: ---

ITEM #312: SURROUND (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #313: BLENDER  
Quantity: One (1)  
Manufacturer: VITAMIX  
Model No.: 036019-ABAB  
Pertinent Data: WITH DOME  
Utilities Req'd: 120V/1PH, 15.0A

ITEM #314: KNOCK BOX  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #301  
Utilities Req'd: ---

ITEM #315: SPARE NUMBER

ITEM #316: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #317: ESPRESSO SYRUP BOTTLE HOLDER (NOT IN CONTRACT)  
Quantity: Two (2)  
Pertinent Data: BY OS&E

ITEM #318: ESPRESSO MACHINE  
Quantity: One (1)  
Manufacturer: SCHAERER  
Model No.: COFFEE ART PLUS  
Pertinent Data: ---  
Utilities Req'd: 208V/1PH, 30.0A; 3/8" CW, 1-1/2" IW

ITEM #319: SPARE NUMBER

ITEM #320: SPARE NUMBER

ITEM #321: ICE MAKER WITH BIN  
Quantity: One (1)  
Manufacturer: SCOTSMAN  
Model No.: UC2024MA-1  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #322: WATER FILTRATION SYSTEM  
Quantity: One (1)  
Manufacturer: SCOTSMAN  
Model No.: AP1-P  
Pertinent Data: FOR ITEM #310  
Utilities Req'd: 3/8" CW

ITEM #323: CUP DISPENSER (NOT IN CONTRACT)  
Quantity: Two (2)  
Pertinent Data: BY VENDOR

ITEM #324: PORTABLE COFFEE DISPENSER  
Quantity: One (1)  
Manufacturer: MICROMATIC  
Model No.: MDD23-E-AMER  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 4.0A

ITEM #325: SPARE NUMBER

ITEM #326: BARISTA BACK COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: (2) 120V/1PH, 20.0A (CONVENIENCE OUTLETS); 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #327: DROP-IN HAND SINK  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-42  
Pertinent Data: WITH SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with gooseneck faucet.  
3. Provide with c fold towel dispenser.  
4. Provide unit with p trap and tail piece.  
5. Provide unit with wrist blade.  
6. Coordinate installation into Item #1501, Back Counter as shown on drawings.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #328: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #327  
Utilities Req'd: ---

ITEM #329: SPARE NUMBER

ITEM #330: SPARE NUMBER

ITEM #331: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #332: COFFEE GRINDER  
Quantity: One (1)  
Manufacturer: BUNN  
Model No.: 35600.002  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 15.0A

ITEM #333: COFFEE BREWER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #334: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: D48N-U  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 2.5A

ITEM #335: SPARE NUMBER

ITEM #336: RAPID COOK OVEN  
Quantity: One (1)  
Manufacturer: TURBOCHEF  
Model No.: BULLET  
Pertinent Data: ---  
Utilities Req'd: 208V/1PH, 16.8A

ITEM #337: CONDIMENT COUNTER  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: (2) 120V/1PH, 20.0A (CONVENIENCE OUTLETS)

ITEM #338: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #353  
Utilities Req'd: ---

ITEM #339: SPARE NUMBER

ITEM #340: SPARE NUMBER

ITEM #341: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #342: NAPKIN DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #343: UTENSIL DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #344: CONDIMENT DISPENSER (NOT IN CONTRACT)  
Quantity: Two (2)  
Pertinent Data: BY OS&E

ITEM #345: SPARE NUMBER

ITEM #346: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #353  
Utilities Req'd: ---

ITEM #347: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #348: SPARE NUMBER

ITEM #349: SPARE NUMBER

ITEM #350: SPARE NUMBER

ITEM #351: DRY STORAGE SHELVING  
Quantity: One (1)  
Manufacturer: METRO  
Model No.: CHROME  
Pertinent Data: FIXED, FIVE TIER  
Utilities Req'd: ---

ITEM #352: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #353: HAND SINK (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: ADVANCE TABCO  
Model No.: 7-PS-68  
Pertinent Data: WITH VENDOR PROVIDED SOAP & TOWEL DISPENSER, EXISTING TO REMAIN  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with gooseneck faucet.  
3. Provide unit with p trap and tail piece.  
4. Provide battery-operated faucet. (K-175 swing spout faucet).  
5. Provide 6 Volt battery to operate electronic sensor.  
6. Provide 12” welded side splash on each side 7-PS-11.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #354: WORK COUNTER WITH SINK  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 20.0A (CONVENIENCE OUTLETS); 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #355: SPARE NUMBER

ITEM #356: REACH-IN REFRIGERATION  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: 1RN  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 5.5A

ITEM #357: REACH-IN FREEZER  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: 2FN  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 9.8A

ITEM #358: SPARE NUMBER

ITEM #359: SPARE NUMBER

ITEM #360: SPARE NUMBER

ITEM #361: REFRIGERATED GRAB-N-GO  
Quantity: Two (2)  
Manufacturer: STRUCTURAL CONCEPTS  
Model No.: B3632  
Pertinent Data: SELF CONTAINED  
Utilities Req'd: 120V/1PH, 16.0A

ITEM #362: MILLWORK SURROUND (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #363: SPARE NUMBER

ITEM #364: SPARE NUMBER

ITEM #365-400: SPARE NUMBERS

**MAIN BAR AREA**

ITEM #401: BAR TOP AND DIE (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #402: UNDERCOUNTER FREEZER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: HB24FS-SD-STK  
Pertinent Data: WITH DRAWERS  
Utilities Req'd: 120V/1PH, 2.4A

ITEM #403: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #404: SODA GUN (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR, CONNECTED TO ITEM #406

ITEM #405: SPARE NUMBER

ITEM #406: SODA GUN HOLDER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS6SGB  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide all stainless steel construction.  
4. Provide top Cover and Manifold Mounting Bracket for both Wunder Bar7 and Schroeder AmericaJ are included on 6” long fillers.  
5. Provide manifold mounts to side panel for easy access and service.  
6. Provide drip cup/cradle mounts to cover.  
7. Provide connection to Item #278, Cocktail Station.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #407: SPEED RAIL  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: SR-S36A  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #408: COCKTAIL STATION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS30IC10  
Pertinent Data: ---  
Utilities Req'd: 1 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-30 Bottle well.  
7. Coordinate installation of Item #1611, Bottle Rail, and Item #1612, Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #409: SPARE NUMBER

ITEM #410: SPARE NUMBER

ITEM #411: DUMP SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12PS-SR  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #412: BOTTLE COOLER (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BC24  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: 120V/1PH, 3.2A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Bottle Cooler shall be self-contained refrigeration.  
3. Provide unit with single access door with lock in lid.  
4. Provide unit with stainless steel interior and exterior.  
5. Provide unit with bin dividers.  
6. Unit shall be provided with heavy-duty cord and plug, coordinate NEMA configuration with electrical contractor.  
7. Coordinate radius curve with the entire bar layout.  
8. Provide the following options and accessories:  
a. Cabinet Finishes  
i. Black Option: Front and ends are black vinyl coated steel (back and bottom galvanized).  
ii. Stainless Steel Option: Front and ends are stainless steel (back and bottom are galvanized).  
iii. All Stainless Steel Option: Front, ends, back and bottom are stainless steel.  
b. Floor Racks.  
c. Bin Dividers.  
d. Interior Light (installed).  
e. Casters.  
f. Speed Rails.  
g. Adjustable Legs.  
h. Bottle Opener and Receiver.  
i. Wine Temperature (specify red or white).  
j. Roller Basket Shelving.  
k. Door Locks.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #413: POS CABINET (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF18POS  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #414: POS SYSTEM (NOT IN CONTRACT) (EXISTING EQUIPMENT)  
Quantity: One (1)  
Pertinent Data: BY OS&E, EXISTING TO BE RELOCATED

ITEM #415: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #416: POS PRINTER (NOT IN CONTRACT) (EXISTING EQUIPMENT)  
Quantity: One (1)  
Pertinent Data: BY OS&E, EXISTING TO BE RELOCATED

ITEM #417: BOTTLE DISPLAY (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12LS  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide a five-tier display step unit, with bottle guards on each step.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #418: SODA GUN (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: ---  
Pertinent Data: CONNECTED TO ITEM #421, EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #419: SPARE NUMBER

ITEM #420: SPARE NUMBER

ITEM #421: SODA GUN HOLDER (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS6SGB  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide all stainless steel construction.  
4. Provide top Cover and Manifold Mounting Bracket for both Wunder Bar7 and Schroeder AmericaJ are included on 6” long fillers.  
5. Provide manifold mounts to side panel for easy access and service.  
6. Provide drip cup/cradle mounts to cover.  
7. Provide connection to Item #278, Cocktail Station.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #422: SPEED RAIL (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: SR-S36A  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #423: COCKTAIL STATION (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS30IC10  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: 1 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-30 Bottle well.  
7. Coordinate installation of Item #1611, Bottle Rail, and Item #1612, Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #424: TRASH UNIT (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #425: SPARE NUMBER

ITEM #426: DUMP SINK (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12PS-SR  
Pertinent Data: WITH RINSER, EXISTING TO BE RELOCATED  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #427: CORNER DRAINBOARD  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: 1" IW

ITEM #428: UNDERCOUNTER FREEZER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: HB24FS-SD-STK  
Pertinent Data: WITH DRAWERS  
Utilities Req'd: 120V/1PH, 2.4A

ITEM #429: SPARE NUMBER

ITEM #430: SPARE NUMBER

ITEM #431: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #432: POS CABINET (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF18POS  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #433: POS SYSTEM (NOT IN CONTRACT) (EXISTING EQUIPMENT)  
Quantity: One (1)  
Pertinent Data: BY OS&E, EXISTING TO BE RELOCATED

ITEM #434: POS PRINTER (NOT IN CONTRACT) (EXISTING EQUIPMENT)  
Quantity: One (1)  
Pertinent Data: BY OS&E, EXISTING TO BE RELOCATED

ITEM #435: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #436: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #437: BOTTLE DISPLAY (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12LS  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide a five-tier display step unit, with bottle guards on each step.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #438: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #439: SPARE NUMBER

ITEM #440: SPARE NUMBER

ITEM #441: SODA GUN (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: ---  
Pertinent Data: CONNECTED TO ITEM #442, EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #442: SODA GUN HOLDER (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS6SGB  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide all stainless steel construction.  
4. Provide top Cover and Manifold Mounting Bracket for both Wunder Bar7 and Schroeder AmericaJ are included on 6” long fillers.  
5. Provide manifold mounts to side panel for easy access and service.  
6. Provide drip cup/cradle mounts to cover.  
7. Provide connection to Item #278, Cocktail Station.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #443: SPEED RAIL (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: SR-S36A  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #444: COCKTAIL STATION (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS30IC10  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: 1 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-30 Bottle well.  
7. Coordinate installation of Item #1611, Bottle Rail, and Item #1612, Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #445: SPARE NUMBER

ITEM #446: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #447: TRASH UNIT (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #448: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #449: SPARE NUMBER

ITEM #450: SPARE NUMBER

ITEM #451: DUMP SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12PS-SR  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #452: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #453: DRAINBOARD (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: 7055A-D  
Pertinent Data: WITH GLASS RACK, EXISTING TO BE RELOCATED  
Utilities Req'd: 1" IW

ITEM #454: CORNER DRAINBOARD  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: 1" IW

ITEM #455: SPARE NUMBER

ITEM #456: GLASSWASHER (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: PKHT24  
Pertinent Data: 180°F, EXISTING TO BE RELOCATED  
Utilities Req'd: 208V/1PH, 33.0A; 1/2" HW, 1" IW, 1" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be provided with built-in 70 degree rise booster heater.  
3. Unit shall be provided with SafetyTemp feature ensures proper temperatures in the final rinse.  
4. Unit shall be provided with built-in detergent and rinse aid pumps.  
5. Provide shop drawings for approval prior to installation.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #457: DRAINBOARD WITH STORAGE CABINET  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12SC  
Pertinent Data: ---  
Utilities Req'd: 1" IW

ITEM #458: HAND SINK (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12HSN  
Pertinent Data: WITH SOAP & TOWEL DISPENSER, EXISTING TO BE RELOCATED  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 15/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide with towel and liquid soap dispenser.  
4. Provide unit with plash guards which shall be 12” high on sides and shall be mounted using stainless steel screws.  
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #459: SPARE NUMBER

ITEM #460: SPARE NUMBER

ITEM #461: TRASH UNIT (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #462: POS CABINET (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF18POS  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #463: POS SYSTEM (NOT IN CONTRACT) (EXISTING EQUIPMENT)  
Quantity: One (1)  
Pertinent Data: BY OS&E, EXISTING TO BE RELOCATED

ITEM #464: POS PRINTER (NOT IN CONTRACT) (EXISTING EQUIPMENT)  
Quantity: One (1)  
Pertinent Data: BY OS&E, EXISTING TO BE RELOCATED

ITEM #465: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #466: BOTTLE DISPLAY  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12LS  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide a five-tier display step unit, with bottle guards on each step.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #467: SODA GUN HOLDER (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS6SGB  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide all stainless steel construction.  
4. Provide top Cover and Manifold Mounting Bracket for both Wunder Bar7 and Schroeder AmericaJ are included on 6” long fillers.  
5. Provide manifold mounts to side panel for easy access and service.  
6. Provide drip cup/cradle mounts to cover.  
7. Provide connection to Item #278, Cocktail Station.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #468: SODA GUN (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: ---  
Pertinent Data: CONNECTED TO ITEM #467, EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #469: SPARE NUMBER

ITEM #470: SPARE NUMBER

ITEM #471: SPEED RAIL (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: SR-S36A  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

ITEM #472: COCKTAIL STATION (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS30IC10  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: 1 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-30 Bottle well.  
7. Coordinate installation of Item #1611, Bottle Rail, and Item #1612, Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #473: TRASH UNIT (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #474: DUMP SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12PS-SR  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #475: SPARE NUMBER

ITEM #476: BOTTLE COOLER (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BC24  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: 120V/1PH, 3.2A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Bottle Cooler shall be self-contained refrigeration.  
3. Provide unit with single access door with lock in lid.  
4. Provide unit with stainless steel interior and exterior.  
5. Provide unit with bin dividers.  
6. Unit shall be provided with heavy-duty cord and plug, coordinate NEMA configuration with electrical contractor.  
7. Coordinate radius curve with the entire bar layout.  
8. Provide the following options and accessories:  
a. Cabinet Finishes  
i. Black Option: Front and ends are black vinyl coated steel (back and bottom galvanized).  
ii. Stainless Steel Option: Front and ends are stainless steel (back and bottom are galvanized).  
iii. All Stainless Steel Option: Front, ends, back and bottom are stainless steel.  
b. Floor Racks.  
c. Bin Dividers.  
d. Interior Light (installed).  
e. Casters.  
f. Speed Rails.  
g. Adjustable Legs.  
h. Bottle Opener and Receiver.  
i. Wine Temperature (specify red or white).  
j. Roller Basket Shelving.  
k. Door Locks.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #477: DRAINBOARD (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: 7055A-D  
Pertinent Data: WITH GLASS RACK, EXISTING TO BE RELOCATED  
Utilities Req'd: 1" IW

ITEM #478: GLASSWASHER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: PKHT24  
Pertinent Data: 180°F RINSE  
Utilities Req'd: 208V/1PH, 33.0A; 1/2" HW, 1" IW, 1" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be provided with built-in 70 degree rise booster heater.  
3. Unit shall be provided with SafetyTemp feature ensures proper temperatures in the final rinse.  
4. Unit shall be provided with built-in detergent and rinse aid pumps.  
5. Provide shop drawings for approval prior to installation.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #479: SPARE NUMBER

ITEM #480: SPARE NUMBER

ITEM #481: DRAINBOARD WITH STORAGE CABINET  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12SC  
Pertinent Data: ---  
Utilities Req'd: 1" IW

ITEM #482: CORNER DRAINBOARD  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: 1" IW

ITEM #483: BOTTLE COOLER (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BC24  
Pertinent Data: EXISTING TO BE RELOCATED  
Utilities Req'd: 120V/1PH, 3.2A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Bottle Cooler shall be self-contained refrigeration.  
3. Provide unit with single access door with lock in lid.  
4. Provide unit with stainless steel interior and exterior.  
5. Provide unit with bin dividers.  
6. Unit shall be provided with heavy-duty cord and plug, coordinate NEMA configuration with electrical contractor.  
7. Coordinate radius curve with the entire bar layout.  
8. Provide the following options and accessories:  
a. Cabinet Finishes  
i. Black Option: Front and ends are black vinyl coated steel (back and bottom galvanized).  
ii. Stainless Steel Option: Front and ends are stainless steel (back and bottom are galvanized).  
iii. All Stainless Steel Option: Front, ends, back and bottom are stainless steel.  
b. Floor Racks.  
c. Bin Dividers.  
d. Interior Light (installed).  
e. Casters.  
f. Speed Rails.  
g. Adjustable Legs.  
h. Bottle Opener and Receiver.  
i. Wine Temperature (specify red or white).  
j. Roller Basket Shelving.  
k. Door Locks.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #484: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #485: SPARE NUMBER

ITEM #486: POS CABINET  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF18POS  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #487: POS SYSTEM (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #488: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #489: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #490: SPARE NUMBER

ITEM #491: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #492: BOTTLE DISPLAY  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12LS  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide a five-tier display step unit, with bottle guards on each step.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #493: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #494: SODA GUN HOLDER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS6SGB  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide all stainless steel construction.  
4. Provide top Cover and Manifold Mounting Bracket for both Wunder Bar7 and Schroeder AmericaJ are included on 6” long fillers.  
5. Provide manifold mounts to side panel for easy access and service.  
6. Provide drip cup/cradle mounts to cover.  
7. Provide connection to Item #278, Cocktail Station.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #495: SPARE NUMBER

ITEM #496: SODA GUN  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: ---  
Pertinent Data: CONNECTED TO ITEM #494  
Utilities Req'd: ---

ITEM #497: SPEED RAIL  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: SR-S36A  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #498: COCKTAIL STATION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS30IC10  
Pertinent Data: ---  
Utilities Req'd: 1 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-30 Bottle well.  
7. Coordinate installation of Item #1611, Bottle Rail, and Item #1612, Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #499: SPARE NUMBER

ITEM #500: SPARE NUMBER

ITEM #501: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #502: DUMP SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12PS-SR  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #503: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #504: TRASH UNIT  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #505: SPARE NUMBER

ITEM #506: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #507: HAND SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12HSN  
Pertinent Data: WITH SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 15/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide with towel and liquid soap dispenser.  
4. Provide unit with plash guards which shall be 12” high on sides and shall be mounted using stainless steel screws.  
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #508: FILLER SECTION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: ---

ITEM #509: SPARE NUMBER

ITEM #510: SPARE NUMBER

ITEM #511: TRASH UNIT  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #512: CORNER DRAINBOARD  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: 1" IW

ITEM #513: SPARE NUMBER

ITEM #514: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #515: SPARE NUMBER

ITEM #516: BACK BAR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #517: SPARE NUMBER

ITEM #518: LOW PROFILE BACK BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BBSLP60  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 5.5A

ITEM #519: SPARE NUMBER

ITEM #520: SPARE NUMBER

ITEM #521: OPEN SHELVING (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #522: BEER DISPENSING TOWER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: 4006-6B  
Pertinent Data: 6 TAP  
Utilities Req'd: ---

ITEM #523: DRIP TROUGH  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: C18645A-GRC  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" IW

ITEM #524: OPEN SHELVING (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #525: SPARE NUMBER

ITEM #526: LOW PROFILE BACK BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BBSLP60  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 5.5A

ITEM #527: LOW PROFILE BACK BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BBSLP60  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 5.5A

ITEM #528: OPEN SHELVING (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #529: SPARE NUMBER

ITEM #530: SPARE NUMBER

ITEM #531: BEER DISPENSING TOWER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: 4006-6B  
Pertinent Data: 6 TAP  
Utilities Req'd: ---

ITEM #532: DRIP TROUGH  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: C18645A-GRC  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" IW

ITEM #533: OPEN SHELVING (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #534: LOW PROFILE BACK BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BBSLP60  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 5.5A

ITEM #535: SPARE NUMBERS

ITEM #536: SERVER STATION (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #537: POS SYSTEM (NOT IN CONTRACT)  
Quantity: Two (2)  
Pertinent Data: BY OS&E

ITEM #538: POS PRINTER (NOT IN CONTRACT)  
Quantity: Two (2)  
Pertinent Data: BY OS&E

ITEM #539: SPARE NUMBER

ITEM #540: SPARE NUMBER

ITEM #541: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #542: SPARE NUMBER

ITEM #543: SPARE NUMBER

ITEM #544: SPARE NUMBER

ITEM #545-600: SPARE NUMBER

**BAR AREA**

ITEM #601: BAT TOP AND DIE (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #602: BOTTLE COOLER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BC24  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 3.2A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Bottle Cooler shall be self-contained refrigeration.  
3. Provide unit with single access door with lock in lid.  
4. Provide unit with stainless steel interior and exterior.  
5. Provide unit with bin dividers.  
6. Unit shall be provided with heavy-duty cord and plug, coordinate NEMA configuration with electrical contractor.  
7. Coordinate radius curve with the entire bar layout.  
8. Provide the following options and accessories:  
a. Cabinet Finishes  
i. Black Option: Front and ends are black vinyl coated steel (back and bottom galvanized).  
ii. Stainless Steel Option: Front and ends are stainless steel (back and bottom are galvanized).  
iii. All Stainless Steel Option: Front, ends, back and bottom are stainless steel.  
b. Floor Racks.  
c. Bin Dividers.  
d. Interior Light (installed).  
e. Casters.  
f. Speed Rails.  
g. Adjustable Legs.  
h. Bottle Opener and Receiver.  
i. Wine Temperature (specify red or white).  
j. Roller Basket Shelving.  
k. Door Locks.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #603: TRASH UNIT  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #604: DUMP SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12PS-SR  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #605: SPARE NUMBER

ITEM #606: SPEED RAIL  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: SR-S36A  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #607: COCKTAIL STATION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS30IC10  
Pertinent Data: ---  
Utilities Req'd: 1 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-30 Bottle well.  
7. Coordinate installation of Item #1611, Bottle Rail, and Item #1612, Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #608: SODA GUN HOLDER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS4SGA  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #609: SPARE NUMBER

ITEM #610: SPARE NUMBER

ITEM #611: SODA GUN  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: ---  
Pertinent Data: CONNECTED TO ITEM #608  
Utilities Req'd: ---

ITEM #612: BOTTLE DISPLAY  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12LS  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide a five-tier display step unit, with bottle guards on each step.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #613: POS CABINET  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF18POS  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #614: POS SYSTEM (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #615: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #616: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #617: HAND SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12HSN  
Pertinent Data: WITH SOAP & TOWEL DISPENSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 15/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide with towel and liquid soap dispenser.  
4. Provide unit with plash guards which shall be 12” high on sides and shall be mounted using stainless steel screws.  
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #618: TRASH UNIT  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #619: SPARE NUMBER

ITEM #620: SPARE NUMBER

ITEM #621: DRAINBOARD WITH STORAGE CABINET  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF24SC-GR  
Pertinent Data: ---  
Utilities Req'd: 1" IW

ITEM #622: GLASSWASHER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: PKHT24  
Pertinent Data: 180°F RINSE  
Utilities Req'd: 208V/1PH, 33.0A; 1/2" HW, 1" IW, 1" DW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be provided with built-in 70 degree rise booster heater.  
3. Unit shall be provided with SafetyTemp feature ensures proper temperatures in the final rinse.  
4. Unit shall be provided with built-in detergent and rinse aid pumps.  
5. Provide shop drawings for approval prior to installation.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #623: DRAINBOARD WITH STORAGE CABINET  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF24SC-GR  
Pertinent Data: ---  
Utilities Req'd: 1" IW

ITEM #624: BOTTLE COOLER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BC24  
Pertinent Data: ---  
Utilities Req'd: 120V/1PH, 3.2A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Bottle Cooler shall be self-contained refrigeration.  
3. Provide unit with single access door with lock in lid.  
4. Provide unit with stainless steel interior and exterior.  
5. Provide unit with bin dividers.  
6. Unit shall be provided with heavy-duty cord and plug, coordinate NEMA configuration with electrical contractor.  
7. Coordinate radius curve with the entire bar layout.  
8. Provide the following options and accessories:  
a. Cabinet Finishes  
i. Black Option: Front and ends are black vinyl coated steel (back and bottom galvanized).  
ii. Stainless Steel Option: Front and ends are stainless steel (back and bottom are galvanized).  
iii. All Stainless Steel Option: Front, ends, back and bottom are stainless steel.  
b. Floor Racks.  
c. Bin Dividers.  
d. Interior Light (installed).  
e. Casters.  
f. Speed Rails.  
g. Adjustable Legs.  
h. Bottle Opener and Receiver.  
i. Wine Temperature (specify red or white).  
j. Roller Basket Shelving.  
k. Door Locks.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #625: SPARE NUMBER

ITEM #626: DUMP SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12PS-SR  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #627: TRASH UNIT  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12BTB  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide removable trim ring.  
4. Provide Rubbermaid gray polyvinyl wastebasket.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #628: SPEED RAIL  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: SR-S36A  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #629: SPARE NUMBER

ITEM #630: SPARE NUMBER

ITEM #631: COCKTAIL STATION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS30IC10  
Pertinent Data: ---  
Utilities Req'd: 1 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-30 Bottle well.  
7. Coordinate installation of Item #1611, Bottle Rail, and Item #1612, Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #632: SODA GUN HOLDER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS4SGA  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #633: SODA GUN  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: ---  
Pertinent Data: CONNECTED TO ITEM #632  
Utilities Req'd: ---

ITEM #634: BOTTLE DISPLAY  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS12LS  
Pertinent Data: ---  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide a five-tier display step unit, with bottle guards on each step.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #635: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #636: POS CABINET  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF18POS  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #637: POS SYSTEM (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #638: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #639: SPARE NUMBER

ITEM #640: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #641: CORNER DRAINBOARD  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: CUSTOM  
Pertinent Data: CUSTOM DESIGN  
Utilities Req'd: 1" IW

ITEM #642: DUMP SINK  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TSF12PS-SR  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" HW, 1-1/2" IW

ITEM #643: SPEED RAIL  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: SR-S36A  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #644: COCKTAIL STATION  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS30IC10  
Pertinent Data: ---  
Utilities Req'd: 1 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-30 Bottle well.  
7. Coordinate installation of Item #1611, Bottle Rail, and Item #1612, Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #645: SPARE NUMBER

ITEM #646: SODA GUN HOLDER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: TS6SGA  
Pertinent Data: ---  
Utilities Req'd: ---

ITEM #647: SODA GUN  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: ---  
Pertinent Data: CONNECTED TO ITEM #646  
Utilities Req'd: ---

ITEM #648: BACK BAR COUNTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #649: SPARE NUMBER

ITEM #650: SPARE NUMBER

ITEM #651: LOW PROFILE BACK BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BBSLP60  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 5.5A

ITEM #652: OPEN SHELVING (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #653: DRIP TROUGH  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: C18645A-GRC  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" IW

ITEM #654: BEER DISPENSING TOWER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: 4006-6B  
Pertinent Data: 6 TAP  
Utilities Req'd: ---

ITEM #655: UNDERCOUNTER FREEZER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: HB24FS-SD-STK  
Pertinent Data: WITH DRAWERS  
Utilities Req'd: 120V/1PH, 2.4A

ITEM #656: OPEN SHELVING (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: MILLWORK / BY GENERAL CONTRACTOR

ITEM #657: DRIP TROUGH  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: C18645A-GRC  
Pertinent Data: WITH RINSER  
Utilities Req'd: 1/2" CW, 1/2" IW

ITEM #658: BEER DISPENSING TOWER  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: 4006-6B  
Pertinent Data: 6 TAP  
Utilities Req'd: ---

ITEM #659: SPARE NUMBER

ITEM #660: LOW PROFILE BACK BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: PERLICK  
Model No.: BBSLP60  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 5.5A

ITEM #661: UNDERCOUNTER REFRIGERATOR  
Quantity: One (1)  
Manufacturer: CONTINENTAL  
Model No.: D27N-U  
Pertinent Data: MOBILE  
Utilities Req'd: 120V/1PH, 6.3A

ITEM #662: ESPRESSO MACHINE  
Quantity: One (1)  
Manufacturer: LA MARZOCCO  
Model No.: LINEA 2 GROUP  
Pertinent Data: 2 GROUP  
Utilities Req'd: 220V/1PH, 26.0A; 1/2" CW, 1" IW

ITEM #663: ESPRESSO GRINDER  
Quantity: One (1)  
Manufacturer: MAZZER  
Model No.: SUPER JOLLY E  
Pertinent Data: ---  
Utilities Req'd: 230V/1PH, 1.5A

ITEM #664: TRASH CHUTE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: ---  
Pertinent Data: PART OF ITEM #648  
Utilities Req'd: ---

ITEM #665: SPARE NUMBER

ITEM #666: TRASH RECEPTACLE  
Quantity: One (1)  
Manufacturer: RUBBERMAID  
Model No.: FG354060GRAY  
Pertinent Data: SLIM JIM  
Utilities Req'd: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have seam-less construction.  
3. Provide 1968468 stainless steel dolly.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.

ITEM #667: POS SYSTEM (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #668: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #669: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #670: SPARE NUMBER

ITEM #671: POS SYSTEM (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #672: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #673: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #674: POS SYSTEM (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #675: COUNTERFEIT CURRENCY DETECTOR (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY VENDOR

ITEM #676: POS PRINTER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #677: POS SYSTEM (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: BY OS&E

ITEM #678: SPARE NUMBER

ITEM #679: SPARE NUMBER

ITEM #680-700: SPARE NUMBERS

**REMOTE BEER SYSTEM AREA**

ITEM #701: BEER SYSTEM (EXISTING EQUIPMENT)  
Quantity: One (1)  
Manufacturer: MICRO MATIC  
Model No.: MMPP4305 PKG  
Pertinent Data: AIR COOLED, EXISTING TO REMAIN  
Utilities Req'd: ---

ITEM #702: SPARE NUMBER

ITEM #703: SPARE NUMBER

ITEM #704: SPARE NUMBER

ITEM #705-800: SPARE NUMBER